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 *************************************************************************************************************************
ÖFFENTLICHE AUSSCHREIBUNG / PUBLIC ANNOUNCEMENT

Purchase and installation of shedding to be made of scaffolding components


**************************************************************************************************************************

The U.S. Consulate General Frankfurt invites you to submit offers for a firm fixed price for:
Das US Konsulat Frankfurt bittet Sie ein Pauschalangebot für die folgenden Leistungen zu übermitteln:


1.	Conditions

The contractor is advised that–

•	Normal US Consulate working hours are 08:00-16:30hrs Monday – Friday.
•	The Principle Contractor who is awarded the project/contract shall be named within this document as the contractor. 
•	The contractor shall familiarize him/herself fully with this specification document and include for all materials, labor and equipment costs to complete the tasks and actions that are specified within this document.
•	The Consulate operates strict security procedures for entry into the building, all tradesmen’s/women’s details shall be provided to the Contracting Officers Representative (COR) a minimum 48 hours before visiting building. 
•	All of his/her employees shall require security clearance before being allowed to work at the Consulate or Government owned/long term leased properties; to obtain clearance each employee shall complete all required security clearance forms. 
•	When working within residential buildings the contractor shall ensure that all doors remain closed/locked at all times and ensure the properties are left secure at the end of each working day.
•	Security at the residential properties shall be the contractor’s responsibility throughout the duration of the project.
•	Access to the property is limited and only with agreement by either the occupant or the COR.
•	No work shall be started or materials ordered until the contractor has received a purchase order for the works or has been given notice by the Contracting Officer.
•	The costs of additional work performed by the contractor not described in this specification and not approved in writing by the U.S. Government shall be borne by the contractor.
•	No work shall be completed on American/German holidays unless by prior arrange/agreement and at no addition costs to the US Government.
•	The contractor is responsible for all site management including all Health & Safety, welfare & first aid facilities, employment/managing/programming of sub-contractors and site security. 
•	The contractor shall provide the Contracting Officers Representative (COR) with all risk assessments and method statements prior to starting on site.
•	The contractor shall provide the COR a detailed program of works mapping each major task, from project start to completion finish.
•	It’s the contractor’s responsibility to ensure that all project tasks specified within the specification/drawings adhere to all HSE guidelines. 
•	Visually display, all health and safety documents and copy of public liability insurance and project specification/drawings. 
•	Where the Contractor considers that the execution of any Order for work will, or is likely to, involve any interference with asbestos-based materials, lead, gas piping or storage containers, pipes conveying steam and any other hazardous substances or installations, he shall immediately stop work and forthwith notify the COR who will give the Contractor further instructions.
•	The contractor shall request a hot works permit prior to starting any soldering/welding work.
•	The contractor shall provide competent a foreman or leading hand on site whilst the project is in progress and he/she shall keep a copy of the specification, visitor log, and necessary Health & Safety logs daily updated, ready for inspection at any time by the “Contracting Officers Representative”.
•	Only competent skilled tradesmen shall be employed to execute all aspects of the works.
•	All work must be executed strictly in accordance with the current Codes of Practice.
•	The contractor shall provide a complete Health & Safety/Operations file for completed works, including all operating instructions and service manuals for all appliances, equipment and materials installed, with details of all guarantees. Include all project COSH data sheets for materials within this document.
•	Complete recycle program for all materials that are to be karted away.
•	All works to be completed in accordance with relevant German/American Standards.
•	The contractor is responsible for their own tools at all times and shall provide a lockable tool/material box for their operative’s tools and materials if/when required.
•	Portables radios or other portable music devices are only allowed at residential buildings if the volume is low and shall not cause any nuisance to neighboring occupants and residents.
•	No Smoking on premises. 


2.	Background

Facility Management proposes to purchase shedding to be made of scaffolding component parts and material and be built as an integrated system to protect the walkways and entrance on 3 sides of the buildings and must comply with German code. The shedding must protect pedestrians at all times.   Scaffolding must have lighting properly lighting the walkway underneath.  
The contractor shall provide the complete service from design and installation of all components.
The contractor shall ensure that they familiarize themselves with the technical specification prior to the arranged site visit.
From notice to proceed the contractor has 30 calendar days to measure, manufacture, install and complete the project.
The property may be occupied during the project so the contractor is to ensure that the resident has full use of the grounds and access to the house whilst the project is ongoing. 
The contractor shall keep a clean site and ensure tools & materials stowed in a safe manner.
3.	Description

Facilities Maintenance is planning to install shedding to be made of scaffolding component parts and material and be built as an integrated system to protect the walkways and entrance on 3 sides of 4 apartment buildings. The shedding must protect pedestrians at all times.  Scaffolding must have lighting properly lighting the walkway underneath. The square meters is 425 sq. per building. 
 

4.	General Requirements/Equipment

1.	All scaffolding components must comply with German code
Alle Gerüstteile benoetigen eine Herstellerzulassung in Deutschland

2.	All scaffolding components must be from the same manufacturer.
Alle Gerüstteile müssen der durch dieGenehmigungsnummer gekennzeichnet sein und vom gleichen Hersteller stammen.

3.	Necessary measures to prevent individuals to climb at the scaffolding
Notwendige Maßnahmen um zu verhindern das Unbefugte auf das Gerüst klettern.

4.	Cost estimate to purchase scaffolding to cover/protect paved walkway, length 55 meter, and entrance walkways in front of buildings. Estimated 275 square meters
Erstellung eines Kaufangebotes fuer ein Gerüst um Fussgänger auf dem Fussweg, sowie die beiden Eingangsbereiche, vor dem Gebäude gegen herabfallende Ziegel zu schützen.

5.	Cost estimate to purchase scaffolding to cover/protect paved walkways, small sides of building. One side, length 15meter, same height and width like scaffolding in front of building.
Erstellung eines Kaufangebotes fuer ein Gerüst um Fußgänger auf dem Fussweg an der Kopfseite des Gebäudes gegen herabfallende Ziegel zu schützen. Länge 15 meter, Höhe und Breite identisch mit Tunnel vor dem Gebäude.

6.	Cost estimate to purchase scaffolding to cover/protect paved walkways, small side of building. Length 15 meter, height 5 meter and width 6 meters.
Erstellung eines Kaufangebotes fuer ein Gerüst um Fußgänger auf dem Fussweg an der Kopfseite des Gebäudes gegen herabfallende Ziegel zu schützen. Länge 15 meter, Höhe 5 meter, Breite 6 meter.

7.	Cost estimate for delivery and installation of dust/safety nets to cover all sides of scaffoldings
Erstellung eines Kaufangebot für die Lieferung und Montage von Sicherheitsnetzen and den Aussenseiten des Gerüsts

8.	Cost estimates  (for Point 5, 6, 7 and 8 )
Erstellung von Angeboten ( fuer Punkt 5, 6, 7 und 8 )


9.	Safety

Contractor and contractor employees must adhere to all US Construction safety including the following:

	Have a dedicated safety coordinator on site at all times.
	Conduct weekly safety meeting and record minutes and submit minutes to COR
	All workers must wear US required Personal Protection Equipment (PPE) including :
o	Hard hats
o	Googles/safety glasses
o	Safety Shoes
o	Hearing protection
o	Protective gloves
o	Dust masks
o	Respirators
	Construction safety plan 
	Crane operations plan
	Provide all material safety data sheets and insure copies are available at project site.

10.	Quality

Once installed, all products shall be checked if fully operational. An approved quality checklist shall be given to the COR after installation. The Government will not be liable for any breakages or damages to materials whilst they are on site and will only accept products once project is completed and snagging completed.


11.	 Installation
Erecting the scaffold must comply with German code
Prüfung durch eine "zur Prüfung befähigte Person" nach Fertigstellung und vor Übergabe an den Benutzer, um den ordnungsgemäßen Zustand festzustellen (Nachweis-Prüfprotokoll).
 

12.	Completion

The contractor shall conduct on site quality checks prior to project completion/acceptance and advise Facility Management Office when product is ready for snagging.

Remove all unused materials and equipment from site. 


13.	Future Maintenance

Provide a full operation manual for all installed equipment, detailing periodic maintenance requirements.



[bookmark: _GoBack]
Shipping terms:
Lieferbedingungen:
Including delivery to the Consulate General Frankfurt.
Inklusive Lieferung an das örtliche Generalkonsulat in Frankfurt

Payment terms:
Zahlungsbedingungen:
Payment terms are to be 30 days after Government acceptance of supplies delivered/
Rechnungsstellung nach Lieferung mit 30 Tagen Zahlungsziel

Request for Quotation Number:
Ausschreibungsnummer:
PR7612640

Due date for quotation: 
Letzter Abgabetermin:
13 September, 2018	

The responsible purchasing agent for this announcement would be:
Der zuständige Ansprechpartner für diese Ausschreibung ist:


Purchasing Agent:  Thomas Petersen
E-Mail: FrankfurtGSOProcurementTeam@state.gov
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