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The U.S. Consulate in Ciudad Juarez, Chihuahua, Mexico is requesting quotes for light fixtures and installation as per specifications below.

 Please submit all quotes no later than July 17th  by 4:00 pm (mountain time) to MaciasG@state.gov. No quotes will be considered after this date and time. Your quote should be valid until September 15th, 2018. For ALL (MX and U.S.) vendors, it is required that you have a current DUNS number, CAGE number and registered in SAM. No quotes can be considered without meeting this criteria. Mexican vendors must quote in pesos unless they  have a U.S. dollar bank account in Mexico. Please include as many specifications as possible for each item as well as your DUNS number with the quote.
Material prices should be quoted separated from the installation cost.
Quantity or item could be decresed or not requested
· 12 pcs, Light Fixture Indy Architectural Recessed Lighting Mod. LC8 P 33LM 40K MVOLT W G4 90CRI EZ1 HW CS with Mounting Hardware PSTEM 36” WPEN
· Installation height: 3.5 to 5.5 meters
· 10 pcs, LED light kit Kim Lighting Mod. ARLED KIT 3 P 70 80L 4K 277
· Installation height: 5.5 meter
· 11 pcs, LED light Lithonia lighting, Mod. KACM LED-30C-530-30K-R5-MVOLT-SRM-DNAXD
· Installation height: 5 meter
· 1 pc, LED light Fixture Lithonia Lighting Mod. DSXPG LED 20C 530 40K T5M MVOLT SLVRD DNAXD
· Installation height: 4.5 meter
· 25 pcs, LED Philips GARDCO, No. Part 101L-16L-700-WW-G1-3-UNV-MGY
· Installation height: 4 meter
· 40 pcs, LED Philips GARDCO, No. Part 101L-16L-700-WW-G1-2-EBPC-UNV-MGY
· Installation height: 4 meter
· 40 pcs, LED Kim Lighting Scarab Mod.  C700S3/9L3KUV-VG
· Installation height: floor level
· 160	pcs LED Hyperikon 18w, T8, 3500K, 841000735R, clear (box 4pcs) (T8)
· Installation height: 3 meter
· 13 pcs LED Rebelle Architectural Lighting, Mod. 2756T-32L-30-277-CL-T3-90-AN
· Installation height: 5 meter
· 15 pcs, LED Rebelle Architectural Lighting, Mod. 2756A2-32L-277-CL-T3-90-AN
· Installation height: 4.5 meter





Installation quote should cover:


· Installation of all fixtures and bulbs, disconnect and remove existing fixture/bulb, Install and connect new fixture/bulb. All labor necessary to move all fixtures/bulbs, installation, place all old fixtures on a location designed inside compound. Consider all fixture change during week working time (8:00 am to 5:00 pm).

The materials could be shipped to the following address. 

From inside the United States:

American Consulate General Ciudad Juarez
9560 Joe Rodriguez Dr. 
Space Border Logistics Corp. 
El Paso, TX 79927-2146

From inside Mexico:
U.S. Consulate General
Paseo de la Victoria #3650
Fracc. Partido Senecú
Ciudad Juárez, Chihuahua, Mexico C.P. 32543
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